{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":24},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"merged":[[0,1,0,2],[0,4,0,6],[1,0,1,6],[3,0,3,6],[14,0,14,6],[22,0,22,6],[27,0,27,6]],"flags":["formulas_cached_only"]}
["contacts:","Chen Sheng 15818512224",null,"Address:","No. 278, Yongfengsheng Industrial Park, \nGuanhu Street, Longhua District, Shenzhen"]
["Shenzhen Huachuang Weishi Technology Co., Ltd"]
["Product model","Product images","Product size (MM)","Parameters","resolution","signal type","notes"]
["USB module"]
["HCU-M121",null,"12*12","Sensor：1/4      \nPixel: 1MP\nFrame rate: 30 fps \nCompression: MJPG/YUY2 \nCompatibility: win， Android\nAudio: Not Supported","1280*720 \n640*480","USB"]
["HCU-M122",null,"12*12","Sensor：1/2.9      \nPixel: 2MP\nFrame rate: 30 fps\nCompression: MJPG/YUY2  \nCompatibility: win， Android\nAudio: support","1920*1080 1280*1024 \n1280*960 \n1280*720 \n640*480","USB"]
["HCU-M124",null,"12*12","Sensor：1/2.8      \nPixel: 4MP\nFrame rate: 25 fps\nCompression: MJPG/YUY3  \nCompatibility: win， Android\nAudio: support","1920*1080 1280*1024 \n1280*960 \n1280*720 \n 640*481","USB"]
["HCU-M125",null,"12*12","Sensor：1/4     \nPixel: 5MP\nFrame rate: 30 fps\nCompression: MJPG/YUY2  \nCompatibility: win， Android\nAudio: support","2560*1440 2592*1944 1920*1080     1280*960 \n1280*720 \n640*480","USB"]
["HCU-M128",null,"12*12","Sensor： 1/3.2 \nPixel: 8MP \nFrame rate: 15 fps Compression: MJPG/YUY2 Compatibility: win， Android Audio: support","3264*2488 2592*1944 1920*1080     1280*960 \n1280*720   ","USB"]
["HCU-M144",null,"14*14","Sensor： 1/2.5 \nPixel: 12MP \nFrame rate: 10 fps Compression: MJPG/YUY2 Compatibility: win， Android Audio: support","4000*3000 3840*2160 2592*1944 1920*1080     1280*720   ","USB"]
["HCU-M282",null,"23 * 23 with 28 * 28 board edges","sensor： 1/2.9 \npixel: 2MP \nframe rate: 30 fps\ncompression: MJPG/YUY2 compatibility: win， Android Audio: support","1920*1080 1280*1024 \n1280*960 \n1280*720   \n640*480","USB"]
["HCU-M382",null,"32 * 32 with 38 * 38 board edge","Sensor： 1/2.9 \nPixel: 2MP \nFrame rate: 30 fps\nCompression: MJPG/YUY2 Compatibility: win， Android Audio: default none, optional","1920*1080 1280*1024 \n1280*960 \n1280*720   \n640*480","USB"]
["HCU-M182",null,"18*42","Sensor： 1/2.9 \nPixel: 2MP\nFrame rate: 30 fps Compression: MJPG/YUY2 Compatibility: win， Android Audio: default none, optional","1920*1080 1280*1024 \n1280*960 \n1280*720   \n640*480","USB"]
["HCU-M81",null,"8*40","Sensor： 1/4 \nPixel: 1MP \nFrame rate: 30 fps\nCompression: MJPG/YUY2 Compatibility: win， Android Audio: default none, optional","1280*720   \n640*480","USB"," "]
["CVBS Module"]
["HCC-M6",null,"6*6","Sensor： 1/6 \nPixel: 300000 pixels\nFrame rate: 50 fps\nAudio: Not Supported \nWorking voltage: 3.3v","640*480","CVBS"]
["HCC-M12",null,"12*12","Sensor： 1/4 \nPixel: 300000 pixels\nFrame rate: 50 fps \nAudio: Not Supported \nWorking voltage: 3.3v","640*480","CVBS(analog signal)"]
["HCC-M23D",null,"23*23","Sensor： 1/3 \nPixel: 700000 pixels\nFrame rate: 50 fps \nAudio: Not Supported\nWorking voltage: 12v","1020*596","CVBS","NVP2090+811"]
["HCC-M23D02",null,"23*23","Sensor： 1/3 \nPixel: 300000 pixels\nFrame rate: 50 fps\nAudio: Not Supported \nWorking voltage: 12v","537*597","CVBS","SONY2463+405ALPure black and white"]
["HCC-M18D",null,"18*36.5","Sensor： 1/3 \nPixel: 700000pixels \nFrame rate: 50 fps\nAudio: Not Supported \nWorking voltage: 12v","1020*596","CVBS","NVP2090+811"]
["HCC-M18C",null,"18*40.2","Sensor： 1/4 \nPixel: 300000 pixels\nFrame rate: 50 fps \nAudio: Not Supported\nWorking voltage: 12v","640*480","CVBS"]
["HCC-CCDM18",null,"18*43","Sensor： 1/3 \nPixel: 700000 pixels\nFrame rate: 50 fps\nAudio: Not Supported\nWorking voltage: 12v","1020*596","CVBS"]
["AHD Module"]
["HCA-M61",null,"6*6","Sensor： 1/4 \nPixel: 1 million \nFrame rate: 25 fps \nAudio:Not Supported\nWorking voltage: 3.3v","1280*720","AHD"]
["HCA-M62",null,"6*6","Sensor： 1/4 \nPixel: 2 million \nFrame rate: 25 fps \nAudio: Not Supported \nWorking voltage: 3.3v","1920*1080","AHD"]
["HCA-M122",null,"12*12","Sensor： 1/2.8 \nPixel: 2 million \nFrame rate: 25 fps\nAudio:Not Supported \nWorking voltage: 3.3v","1920*1080","AHD","UTC"]
["HCA-M182",null,"18*38","Sensor： 1/2.8 \nPixel: 2 million \nFrame rate: 25 fps\nAudio: Not Supported Working voltage: 12v","1920*1080","AHD","UTC"]
["Network Module"]
["HCW-M183",null,"18*42","Sensor： 1/2.9 \nPixel: 3 million \nFrame Rate: 25 fps\nAudio: support \nWorking voltage: 12v"," 1920*1080","WIFI"]
["HCW-M182",null,"18*38.2","Sensor： 1/2.8 \nProtocol: ONVIF \nPixel: 4 million \nFrame rate: 25 fps \nAudio: Not Supported Working Voltage: 12v","2560*1440 \n2304*1296 \n1920*1080","Network RJ45"]
["HCW-M133",null,"13*70","Sensor： 1/2.9 \nPixel: 4 million \nFrame rate:25 fps\nAudio: Not Supported \nWorking Voltage: 5V","1920*1080","WIFI"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}